*Priloga 5A*

*Appendix 5A*

**KAKOVOST USKLADIŠČENEGA NMB 95:**

**THE QUALITY OF STORED UNLEADED GASOLINE 95:**

1. V skladišču Petrol, d.d., Dunajska cesta 50, 1000 Ljubljana, na lokaciji SND Rače, Turnerjeva ulica 24, 2313 Fram, se v rezervoarju R 12 nahaja neosvinčen motorni bencin super 95, kakovosti skladno s standardom SIST EN 228 za poletno obdobje.

Ponudniki lahko v roku do oddaje ponudb ob vnaprejšnjem dogovoru s skladiščnikom odvzamejo vzorce blaga iz omenjenih rezervoarjev in izvedejo analizo na lastne stroške.

1. In the storage facility Petrol, d.d., Dunajska cesta 50, 1000 Ljubljana, location SND Rače, Turnerjeva ulica 24, 2313 Fram in the tank R 12 gasoline is stored, quality in accordance with the standard SIST EN 228, summer grade.

Provided that a prior agreement with the storage operator is reached, the tenderers may take samples of the petroleum products from the oil tanks and have the analysis performed at their expense before the expiration of the deadline for the submission of their tenders.

**KAKOVOST DOBAVLJENEGA GORIVA:**

**THE QUALITY OF DIESEL FUEL:**

1. Kakovost: dizelsko gorivo, skladno s standardom SIST EN 590 za zimsko obdobje, brez biogoriv.
2. Quality: ddiesel fuel, SIST EN 590, winter grade, without biofuels.